**Capture image using OV7670 and Arduino-uno**

1. Connection between OV7670 and Arduino – refer “fig1OV7670arduino.png”.

2. Arduino Code- Refer Arduino file “image\_capture”. Upload it selecting the COM

Port.

3. Java Code – There are 5 zip-files for 5 types of COM Port (COM\_JAVA1….)

- Extract the zip file according to COM port

- Paste the folder “code” in

Local Disk > Program Files > Java > jdk1.8.0\_74 > bin

* Open command prompt and go to the folder

Local Disk > Program Files > Java > jdk1.8.0\_74 > bin

- Run the Java Code using “java code.SimpleRead”.